SIMULATION TEST [L8, LF, L3]

id0102a1100600

• The simulation test items for the fuel and emission control systems are as shown in the table below.

Simulation item table

×: Applied
—: Not applied

Simulation item | Applicable component | Operation | Test condition | PCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
ACCS | A/C relay | ON or OFF | × | × | 1I
ALTF | Generator field coil control duty value | ON or OFF | — | × | 2AI
EVAPCP | Purge solenoid valve | For purge solenoid valve: Actuated by any duty value (0—100%) | × | × | 2C
FAN1 | Fan1 control signal | ON or OFF | × | × | 1M
FAN2 | Fan2 control signal | ON or OFF | × | × | 1R
FAN3 | Fan3 control signal | ON or OFF | × | × | 1R
FP | Fuel pump relay | ON or OFF | × | × | 1H*1, 1G*2
FUELPW1 | Fuel injection duration | Actuated +50%— -50% fuel injection time | — | × | 2AZ, 2BB, 2BC, 2BD
GENVDSD | Generator voltage desired | Actuated by any voltage of the of the generator | — | × | —
HTR11 | A/F sensor | ON or OFF | × | × | 2BG
HTR12 | HO2S | ON or OFF | × | × | 2BE
IASV*4 | Variable intake air shutter valve | ON or OFF | × | × | 2J
IMRC | Variable tumble control solenoid control signal in PCM | ON or OFF | × | × | 2I
IMTV*3 | Variable intake-air system (VIS) control solenoid control signal in PCM | ON or OFF | × | × | 2J
INJ#1 | Fuel injector (Cylinder No.1) | ON or OFF | — | × | 2BB
INJ#2 | Fuel injector (Cylinder No.2) | ON or OFF | — | × | 2BC
INJ#3 | Fuel injector (Cylinder No.3) | ON or OFF | — | × | 2BD
INJ#4 | Fuel injector (Cylinder No.4) | ON or OFF | — | × | 2AZ
SEGRP | EGR valve (stepping motor) | Actuated by any stepping value (0—60 steps) | × | × | 2G, 2H, 2K, 2L
TEST | — | ON or OFF | × | × | —
VT DUTY1 Wt | Oil control valve | For oil control valve: Actuated by any duty value (0—100%) | × | × | 2E

*1 :With immobilizer system
*2 :Without immobilizer system
*3 :L3
*4 :LF, L3