#
NO.1 DISPLAY SCREEN DOES NOT OPEN EVEN IF THE IGNITION SWITCH IS TURNED TO THE ACC POSITION.

id0903e8801700

1 | Display screen does not open even if the ignition switch is turned to the ACC position.
POSSIBLE CAUSE | • Open or short circuit in power supply (B+ or ACC) wiring harness or burnt fuse • Open or short circuit in GND wiring harness • LCD unit malfunction • Poor connection of LCD unit connector, terminal damage • Short circuit in car-navigation control signal wiring harness Caution • Forcibly opening/closing, or placing an object on the display may cause the display screen to become inoperable.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Turn the ignition switch to the ACC position. • Press the OPEN/CLOSE button on the LCD unit. • Does the display screen open? | Yes | The system is normal. Note • If the display screen is closed by pressing the OPEN/CLOSE button of the LCD unit with the ignition switch at the ACC position, the display screen will remain closed when the ignition switch is turned to the ACC position again.
No | Go to the next step.
2 | • Turn the ignition switch to the LOCK position. • Inspect the following fuses: - RADIO 15 A fuse - ROOM 15 A fuse • Are the fuses damaged? | Yes | Go to the next step.
No | • Replace with the appropriate standard fuse. - If the fuse is melted, inspect the wiring harness for short to ground. Repair or replace the wiring harness, then replace the fuse.
3 | • Remove the car-navigation control switch. • Disconnect the car-navigation control switch connector (6-pin). • Turn the ignition switch ACC position. • Inspect the voltage between the car-navigation control switch wiring harness side connector (6-pin)terminal A (ACC) and F (GND). • Is the voltage B+? | Yes | Go to the Step 5.
No | Go to the next step.
4 | • Turn the ignition switch LOCK position. • Inspect for continuity between terminal A (ACC) and F (GND) at the car-navigation control switch wiring harness side connector. • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the suspect wiring harness. Replace the LCD unit. (See LCD UNIT REMOVAL/INSTALLATION.) (ACC protector circuit inside LCD unit is broken.)
5 | • Remove the LCD unit. (See LCD UNIT REMOVAL/INSTALLATION.) • Inspect the connection of the LCD unit connector (24-pin). • Is the connector securely connected? | Yes | Go to the next step.
No | Securely connect the LCD unit connector (24-pin).
6 | • Disconnect the LCD unit connector (24-pin). • Inspect both LCD unit connector and wiring harness-side connector for poor connection (such as damaged/pulled-out pins, corrosion). • Are all the pins normal? | Yes | Go to the next step.
No | If the LCD unit connector is wrong: Replace the LCD unit. (See LCD UNIT REMOVAL/INSTALLATION.) If the wiring harness-side connector is wrong: Repair or replace the pins and/or the connector.
7 | • Inspect the voltage between LCD unit wiring harness-side connector (24-pin) terminal Q (B+) and P (GND) • Is the voltage B+? | Yes | Go to the next step.
No | Inspect the suspect wiring harness, then repair or replace the wiring harness.
8 | • Turn the ignition switch to the ACC position. • Inspect the voltage between LCD unit wiring harness-side connector (24-pin) terminal O (ACC) and P (GND). • Is the voltage B+? | Yes | Replace the LCD unit. (See LCD UNIT REMOVAL/INSTALLATION.)
No | Inspect the suspect wiring harness, then repair or replace the wiring harness.