#
NO.23 TRANSAXLE OVERHEATS [FS5A-EL]

id050308802800

23 | Transaxle overheats
DESCRIPTION | • Burnt smell emitted from transaxle. • Smoke emitted from transaxle.
POSSIBLE CAUSE | • The malfunction is restricted to the hindrance of coolant at the oil cooler. In addition, overheating of the transaxle may be caused by a malfunction of the transaxle fluid temperature sensor. 1. Burnt (TCC) • Line pressure low • Control valve body malfunction • Accelerator cable mis-adjustment 2. Oil cooler malfunction (Foreign material mixed in ATF) 3. Transaxle fluid temperature sensor malfunction 4. Excessive amount of ATF 5. Torque converter malfunction Note • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Inspect for bending, damage, corrosion or kinks of the oil cooler pipes. Are oil cooler pipes normal? | Yes | Go to the next step.
No | Replace any malfunctioning parts.
2 | Perform the stall test. (See Stall Test.) Is the stall speed normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts.
3 | Inspect the value at the following PCM PID using the WDS or equivalent. (See PCM INSPECTION [L8, LF, L3].) • APP • TP REL Is the PID value normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts.
4 | Disconnect the TCM connector. Is the resistance between the ground terminal at the TCM connector and the body ground less than 5.0 ohms? | Yes | Go to the next step.
No | Repair the open ground circuit. Reconnect the TCM.
5 | Inspect the LPS PID value. Is the LPS PID value normal? (See TCM INSPECTION [FS5A-EL].) | Yes | Overhaul the control valve body and repair or replace any malfunctioning parts. (See ATX workshop manual [FS5A-EL].) If any problem remains, overhaul the transaxle and repair or replace any malfunctioning parts. (See ATX workshop manual [FS5A-EL].)
No | Repair or replace any malfunctioning parts.
6 | • Verify the test results. - If normal, return to the diagnostic index to service any additional symptoms. - If the malfunction remains, inspect the related Service information and perform repair or diagnosis. • If the vehicle is repaired, troubleshooting is completed. • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.