#
WINDSHIELD WIPER MOTOR INSPECTION

id091900475000

## L.H.D.

1. Disconnect the windshield wiper motor connector.

2. Connect battery positive voltage to terminal E or D and ground to terminal B, and inspect the operation of the windshield wiper motor as indicated below.

Terminal | Operation
--- | ---
E | High
D | Low

3. Disconnect battery positive voltage from terminal E of the motor while the wipers are operating.

4. Verify that the wipers do not stop in the park position.

5. Short between the motor terminals A and D and connect battery positive voltage to the motor terminal C.

6. Verify that the wipers operate at low speed again, then stop in the park position.

  • If there is any malfunction, replace the windshield wiper motor.

## R.H.D.

1. Disconnect the windshield wiper motor connector.

2. Connect battery positive voltage to terminal B or A and ground to terminal D, and inspect the operation of the windshield wiper motor as indicated below.

Terminal | Operation
--- | ---
B | High
A | Low

3. Disconnect battery positive voltage from terminal B of the motor while the wipers are operating.

4. Verify that the wipers do not stop in the park position.

5. Short between the motor terminals E and A and connect battery positive voltage to the motor terminal C.

6. Verify that the wipers operate at low speed again, then stop in the park position.

  • If there is any malfunction, replace the windshield wiper motor.