#
HEADLIGHT BULB REMOVAL/INSTALLATION

id091800464100

## Low-beam

### Halogen type

1. Disconnect the negative battery cable.

2. Remove the fasteners, then pull back the mudguard.

3. Remove in the order indicated in the table.

1 | Cover
2 | Connector
3 | Headlight bulb (See Headlight bulb removal note.)

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

4. Install in the reverse order of removal.

### Headlight bulb removal note

1. Release the bulb pressing wire to remove the headlight bulb.

### Discharge type

  Caution

  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the "Discharge headlight service warnings." (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

1. Disconnect the negative battery cable.

2. Remove the fasteners, then pull back the mudguard.

3. Remove in the order indicated in the table.

1 | Cover
2 | Connector
3 | Bulb cover
4 | Discharge headlight bulb

  Caution

  • A bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

4. Install in the reverse order of removal.

## High-beam

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

1 | Cover
2 | Connector
3 | Headlight bulb (See Headlight bulb removal note.)

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

3. Install in the reverse order of removal.

### Headlight bulb removal note

1. Release the bulb pressing wire to remove the headlight bulb.