#
VALVE MECHANISM OUTLINE [L8, LF, L3]

id0110a1120000
• There are two intake ports and two exhaust ports each cylinder. Totally 16 valves are directly driven by two camshafts.
• The variable valve timing mechanism, which insures the best valve timing depending on the drive condition by constantly changing the phase of the intake port side camshaft, has been adopted for the LF engine models and L3 engine models.