#
REVERSE IDLER GEAR COMPONENTS DISASSEMBLY/ASSEMBLY

id051500810500

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Roll pin
2 | Reverse idler gear support
3 | Washer
4 | Reverse idler gear
5 | Washer
6 | Reverse clutch hub sleeve
7 | Synchronizer key spring
8 | Reverse synchronizer ring
9 | Reverse idler gear
10 | Friction damper
11 | Reverse idler gear shaft
12 | Needle bearing
13 | Thrust washer (See Thrust Washer Assembly Note.)
14 | Clip

## Thrust Washer Assembly Note

1. Align the tabs of the friction damper and thrust washer and assemble.

2. Measure the dimension A as shown in the figure.

  • If not within the specification, select a suitable thrust washer from the table below so that the dimension is within the specification.

Reverse idler gear component dimension

  57.0-57.5 mm {2.244-2.263 in}

Reverse thrust washer thickness (mm {in})

2.04 {0.080} | 2.24 {0.088}
2.09 {0.082} | 2.29 {0.090}
2.14 {0.084} | 2.34 {0.092}
2.19 {0.086} | 2.39 {0.094}