#
JOINT SHAFT DISASSEMBLY/ASSEMBLY [L8, LF, L3]

id0313008014b4

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Joint shaft (See Joint Shaft Disassembly Note) (See Joint Shaft Assembly Note)
2 | Dust seal (Differential side) (See Dust Seal (Differential Side), Bearing Disassembly Note) (See Dust Seal (Differential Side) Assembly Note.)
3 | Bearing (See Dust Seal (Differential Side), Bearing Disassembly Note.) (See Bearing Assembly Note)
4 | Dust seal (Wheel side) (See Dust Seal (Wheel Side) Assembly Note)
5 | Bracket

## Joint Shaft Disassembly Note

1. Disassemble the joint shaft using the SST.

## Dust Seal (Differential Side), Bearing Disassembly Note

### When the bearing remains on the bracket

1. Remove the bearing and the dust seals (both differential side and wheel side) using the SSTs.

### When the bearing remains on the shaft

1. Remove the bearing from the joint shaft using the SST.

## Dust Seal (Wheel Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new dust seal (wheel side) using the SSTs.

## Bearing Assembly Note

1. Install the new bearing using the SSTs.

## Dust Seal (Differential Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new dust seal (differential side) using a steel plate and the SSTs.

## Joint Shaft Assembly Note

1. Assemble the joint shaft using a press and the SST.