CYLINDER HEAD DISASSEMBLY (I)

id011000500400

1. Disassemble in the order indicated in the table.

e6u110zeb024

1 | Camshaft sprocket, Variable valve timing actuator (See Camshaft Sprocket, Variable Valve Timing Actuator Disassembly Note.)
2 | OCV
3 | Camshaft cap (See Camshaft Cap Disassembly Note.)
4 | Camshaft
5 | Tappet (See Tappet Disassembly Note.)
6 | Cylinder head bolt
7 | Cylinder head (See Cylinder Head Disassembly Note.)
8 | Cylinder head gasket

Camshaft Sprocket, Variable Valve Timing Actuator Disassembly Note

1. Before removing the camshaft, hold the camshaft using a wrench on the cast hexagon and loosen the camshaft sprocket installation bolt.

b3e0110e058

Camshaft Cap Disassembly Note

1. Before removing the camshaft cap, Inspect the camshaft end play. (See CAMSHAFT INSPECTION.)

  Note
  • Determine the position of each removed camshaft cap.

2. Loosen the camshaft cap bolts in two to three passes in the order shown in the figure and remove the camshaft caps.

e6u110zeb001

Tappet Disassembly Note

  Note
  • Determine the position of each removed tappet.

Cylinder Head Disassembly Note

1. Loosen the cylinder head installation bolts in two to three passes in the order shown in the figure and remove them.

b3e0110e059