#
PARKING BRAKE (LEVER TYPE) REMOVAL/INSTALLATION

id041200901900

1. Remove the center console. (See CONSOLE REMOVAL/INSTALLATION.)

2. Remove the rear seat cushion (4SD) or rear seat (5HB, Wagon). (See REAR SEAT REMOVAL/INSTALLATION [EXCEPT WGN (4WD)].) (See REAR SEAT REMOVAL/INSTALLATION [WGN (4WD)].)

3. Remove the tire house trim. (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

4. Remove the propeller shaft. (See PROPELLER SHAFT REMOVAL/INSTALLATION [A26MX-R].)

5. Remove the exhaust pipe bracket.

6. Remove the insulator.

7. Remove in the order indicated in the table.

8. Install in the reverse order of removal.

9. Adjust the parking brake stroke. (See PARKING BRAKE (LEVER TYPE) ADJUSTMENT.)

.

1 | Parking brake switch
2 | Adjusting nut
3 | Parking brake lever
4 | Clip
5 | Parking brake cable