#
SEAT WARMER UNIT INSPECTION

id091300716200

1. Remove the front seat. (See FRONT SEAT REMOVAL/INSTALLATION.)

2. Remove the seat cushion trim.

3. While inspecting for continuity between the terminals A and B of the connector, use a dryer to warm the thermostat of the seat warmer unit on seat cushion.

4. When the indication on the ohmmeter is no continuity, turn off the dryer, then use a thermometer to measure the temperature of the thermostat.

5. Verify that the temperature is approximately 29 °C {84 °F}.

6. Verify that there is continuity between the terminals of seat warmer unit's connector using an ohmmeter when temperature drops to approximately 20 °C {68 °F}.