#
REAR OIL SEAL REPLACEMENT [MZR-CD (RF Turbo)]

id0110f1800900

1. Remove the flywheel. (See CLUTCH UNIT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove the rear oil seal.

  (1) Cut the oil seal lip using a razor knife.
  (2) Remove the oil seal using a screwdriver protected with a rag.

3. Install a new rear oil seal using the following procedure.

  (1) Apply clean engine oil to the oil seal lip.
  (2) Push the oil seal slightly in by hand.
  (3) Tap the oil seal in evenly using the SST and a hammer.
Pushing distance of the rear oil seal (from the edge of the rear cover)

  0-0.5 mm {0-0.019 in}