#
INTAKE SHUTTER VALVE/EGR VALVE INITIALIZATION [MZR-CD (RF Turbo)]

id0140f1445200

1. Connect the WDS or equivalent to DLC-2.

2. Set up the WDS or equivalent (including the vehicle recognition).

3. Select "Powertrain".

4. Select "ETB / EGR Initialization" and perform procedures according to directions on the WDS or equivalent screen.

5. Retrieve DTC's using the WDS or equivalent, then verify that DTCs are present.

  • If a DTC is present, perform the applicable DTC inspection.