#
DSC INDICATOR LIGHT OPERATION

id041500102300
• When the DSC and CAN system is normal, the DSC indicator light illuminates for 2.4 s when the ignition switch is at ON, and goes out, checking the light function. When the system is malfunctioning, the DSC indicator light remains illuminated.
• When DSC and TCS are operating, the DSC indicator light operates as follows:

DSC indicator light operation table

Item | DSC indicator light
--- | ---
TCS, DSC non-operation | Not illuminated
TCS operation | Flashes (0.5 s intervals)
DSC operation | Flashes (0.5 s intervals)

1 | DSC indicator light