#
REAR DOOR UNIT REMOVAL/INSTALLATION

id091100800600

1. Remove the rear door glass. (See REAR DOOR GLASS REMOVAL/INSTALLATION.)

2. Remove the inner handle. (See INNER HANDLE REMOVAL/INSTALLATION.)

3. Remove the rear door speaker. (See REAR DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Disconnect the power window motor connector, and power door lock actuator connector.

5. Remove the rear door harness from the rear door module.

6. Remove the bolts.

7. Remove the rear door lock actuator hook from the rear door module.

8. Pull the rear door unit slightly towards you, and while keeping the power window regulator or manual window regulator from catching on the door, remove the door unit from the door.

9. Pull out the inner handle cable and door lock knob cable from the hole.

10. For power window system-equipped vehicles, remove the power window motor and power window regulator from the door unit. For manual window system-equipped vehicles, remove the regulator handle and manual window regulator.

11. Install in the reverse order of removal.