#
TRUNK LID DISASSEMBLY/ASSEMBLY

id091000407700

1. Disconnect the negative battery cable.

2. Remove the trunk lid trim.

3. To remove the trunk lid outer handle and trunk lid key cylinder, remove the rear finisher.

4. Disassemble in the order indicated in the table.

5. Assemble in the reverse order of disassembly.

1 | Trunk Lid latch and lock actuator
2 | Trunk Lid outer handle
3 | Trunk Lid key cylinder
4 | Clip
5 | Stopper
6 | Trunk Lid weatherstrip
7 | Trunk Lid