#
REQUEST SWITCH REMOVAL/INSTALLATION

id0914z6440000

## Deiver-side/passenger-side

1. Disconnect the negative battery cable.

2. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove the front outer handle. (See FRONT OUTER HANDLE REMOVAL/INSTALLATION.)

4. Remove the screws A, then remove the handle seat and plate.

5. Remove screw B, then remove the request switch.

6. Install in the reverse order of removal.

## Trunk LId/liftgate

1. Disconnect the negative battery cable.

2. Remove the rear finisher. (See REAR FINISHER REMOVAL/INSTALLATION.)

3. Remove the screws, then remove the request switch.

4. Install in the reverse order of removal.