#
FUEL INJECTOR CODE PROGRAM [MZR-CD (RF Turbo)]

id0140f1809900

  Note

  • Regarding the Injector Calibration Code, if the fuel injector is newly replaced, the PCM records a DTC (P1675 and P1676) and illuminates the malfunction indicator lamp even if there is no malfunction. Therefore, if the fuel injector is replaced, program the injector calibration code (rank number) in the PCM using the following procedure.

1. Connect the WDS or equivalent to DLC-2.

2. Set up the WDS or equivalent (including the vehicle recognition).

3. Select "Module Programming".

4. Select "Programmable Parameters".

5. Select "Injector Correction Factors" and perform procedures according to directions on the WDS or equivalent screen.

6. Retrieve DTC's using the WDS or equivalent, then verify that DTCs are present.

  • If a DTC is present, perform the applicable DTC inspection.