#
REAR WASHER NOZZLE REMOVAL/INSTALLATION [5HB]

id0919004767a3

1. Disconnect the negative battery cable.

2. Remove the liftgate upper trim. (See LIFTGATE UPPER TRIM REMOVAL/INSTALLATION [5HB].)

3. Remove the rear washer hose from the rear washer nozzle.

4. Compress the tabs of the rear washer nozzle.

5. Pull the rear washer nozzle out to remove it.

6. Install in the reverse order of removal.

7. Adjust the rear washer nozzle. (See REAR WASHER NOZZLE ADJUSTMENT [5HB].)