#
NO.27 GEAR POSITION INDICATOR LIGHT DOES NOT ILLUMINATE IN M RANGE [JA5AX-EL]

id050305803200

27 | Gear position indicator light does not illuminate in M range
DESCRIPTION | • Gear position indicator light in instrument cluster does not illuminate in M range and ignition switch at on.
POSSIBLE CAUSE | • M range switch, gear position indicator light or related wiring harness malfunction. Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Are other indicator lights illuminated with ignition switch on? | Yes | Go to next step.
No | Inspect meter fuse.
2 | • Inspect MNL SW PID value using WDS or equivalent. • Are these PIDs okay? | Yes | Inspect instrument cluster.
No | Inspect M range switch. If M range switch is okay, inspect for continuity between M range switch and TCM terminal 1AA.
3 | • Verify test results. - If okay, return to diagnostic index to service any additional symptoms. - If malfunction remains, inspect related Service Informations and perform repair or diagnosis. • If vehicle repaired, troubleshooting completed. • If vehicle not repaired or additional diagnostic information not available, replace TCM.