#
FUEL FILTER COMPONENT DISASSEMBLY/ASSEMBLY [MZR-CD (RF Turbo)]

id0114f1777900

1. Disassemble in the order indicated in the table.

1 | Priming pump
2 | Fuel filter (See Fuel Filter Installation Note)
3 | Fuel warmer (Cold District Specification)
4 | Drain plug

2. Assemble in the reverse order of removal.

## Fuel Filter Installation Note

1. Apply a small amount of fuel to the fuel filter O-ring.

2. Tighten the fuel filter approx. 3/4 by hand after the O-ring contacts the priming pump.