#
DSC ON-BOARD DIAGNOSIS

id040200807400

## On-Board Diagnostic (OBD) Test Description

• The OBD test inspects the integrity and function of the DSC and outputs the results when requested by the specific tests.
• On-board diagnostic test also:

  - Provides a quick inspection of the DSC usually performed at the start of each diagnostic procedure.
  - Provides verification after repairs to ensure that no other faults occurred during service.

• The OBD test is divided into 3 tests:

  - Read/clear diagnostic results, PID monitor and record and active command modes.

### Read/clear diagnostic results

  • This function allows you to read or clear DTCs in the DSC HU/CM memory.

### PID/data monitor and record

  • This function allows you to access certain data values, input signals, calculated values, and system status information.

### Active command modes

  • This function allows you to control devices through the WDS or equivalent.

## Reading DTCs Procedure

1. Connect WDS or equivalent to the vehicle DLC-2 connector.

2. Retrieve DTC by WDS or equivalent.

## Clearing DTCs Procedures

1. After repairs have been made, perform the DTCs reading procedure.

2. Erase DTC by WDS or equivalent.

3. Ensure that the customer's concern has been resolved.

## PID/Data Monitor and Record Procedure

1. Connect WDS or equivalent to the vehicle DLC-2 connector.

2. Access and monitor PIDs by WDS or equivalent.

## Active Command Modes Procedure

  Note

  • When driving, the ABS motor and each valve automatically turn ABS_POWER on, and then each command on. ABS_POWER regulates the power supply for the ABS motor and 8 valves.

1. Connect WDS or equivalent to the vehicle DLC-2 16-pin connector.

2. Turn the ignition switch to ON (Engine OFF) or start engine.

3. Activate active command modes using WDS or equivalent.

## DTC Table

DTC | Diagnosis system component | Page
--- | --- | ---
WDS or equivalent
B1318 | DSC power supply | (See DTC B1318 [DSC].)
B1342 | DSC HU/CM | (See DTC B1342 [DSC].)
B1483 | Brake switch signal | (See DTC B1483, B1484, B1486 [DSC].)
B1484 | Brake switch signal | (See DTC B1483, B1484, B1486 [DSC].)
B1486 | Brake switch signal | (See DTC B1483, B1484, B1486 [DSC].)
B1627 | Reverse signal | (See DTC B1627 [DSC].)
B2477 | Module configuration | (See DTC B2477 [DSC].)
C1095 | Motor relay, pump motor | (See DTC C1095, C1096 [DSC].)
C1096 | Motor relay, pump motor | (See DTC C1095, C1096 [DSC].)
C1119 | Engine control system | (See DTC C1119 [DSC].)
C1125 | Brake fluid level sensor | (See DTC C1125 [DSC].)
C1140 | DSC HU/CM (pump) | (See DTC C1140 [DSC].)
C1145 | Right front ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1148 | Right front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1155 | Left front ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1158 | Left front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1165 | Right rear ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1168 | Right rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1175 | Left rear ABS wheel-speed sensor | (See DTC C1145, C1155, C1165, C1175 [DSC].)
C1178 | Left rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1186 | Fail-safe relay | (See DTC C1186, C1266 [DSC].)
C1194 | Left front pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1198 | Left front pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1210 | Right front pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1214 | Right front pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1233 | Left front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1234 | Right front ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1235 | Right rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1236 | Left rear ABS wheel-speed sensor/sensor rotor | (See DTC C1148, C1158, C1168, C1178, C1233, C1234, C1235, C1236 [DSC].)
C1242 | Left rear pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1246 | Right rear pressure reduction solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1250 | Left rear pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1254 | Right rear ABS pressure retention solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1266 | Fail-safe relay | (See DTC C1186, C1266 [DSC].)
C1280 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1400 | Right front traction switch solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1410 | Left front traction switch solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1414 | DSC HU/CM | (See DTC C1414 [DSC].)
C1507 | DSC control | (See DTC C1507, C1508 [DSC].)
C1508*1 | DSC control | (See DTC C1507, C1508 [DSC].)
C1510 | Right front solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1511 | Left front solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1512 | Right rear solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1513 | Left rear solenoid valve, motor or ABS wheel-speed sensor/sensor rotor | (See DTC C1510, C1511, C1512, C1513 [DSC].)
C1730 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1949*2 | Combined sensor | (See DTC C1949, C1950 [DSC].)
C1950*2 | Combined sensor | (See DTC C1949, C1950 [DSC].)
C1951 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1952 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
C1953 | Brake fluid pressure sensor | (See DTC C1953, C1954 [DSC].)
C1954 | Brake fluid pressure sensor | (See DTC C1953, C1954 [DSC].)
C1955 | Steering angle sensor | (See DTC C1955, C1956 [DSC].)
C1956 | Steering angle sensor | (See DTC C1955, C1956 [DSC].)
C1957 | Right front stability control solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1958 | Left front stability control solenoid valve | (See DTC C1194, C1198, C1210, C1214, C1242, C1246, C1250, C1254, C1400, C1410, C1957, C1958 [DSC].)
C1959 | Combined sensor | (See DTC C1280, C1730, C1951, C1952, C1959 [DSC].)
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0100 | Communication error to PCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0101*3 | Communication error to TCM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0114*2 | Communication error to 4WD control module | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0155 | Communication error to instrument cluster | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U2511*2 | Abnormal message from 4WD control module | (See DTC U2511 [DSC].)

  *1 :
Only vehicles with 2WD
  *2 :
Only vehicles with 4WD
  *3 :
Only vehicles with ATX

## PID/DATA Monitor Table

PID Name (Definition) | Unit/Condition | Condition/Specification | Action | DSC HU/CM terminal
--- | --- | --- | --- | ---
ABS_LAMP (ABS warning light driver output state) | On/Off | • ABS warning light is illuminated: ON • ABS warning light is not illuminated: Off | Inspect ABS warning light. | -
ABSLF_I (Left front ABS pressure retention solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSLF_O (Left front ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSLR_I (Left rear ABS pressure retention solenoid valve output state) | On/Off | • During ABS or EBD control: On/Off (solenoid valve is activated/deactivated) • Not ABS and EBD control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSLR_O (Left rear ABS pressure reduction solenoid valve output state) | On/Off | • During ABS or EBD control: On/Off (solenoid valve is activated/deactivated) • Not ABS and EBD control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSRF_I (Right front ABS pressure retention solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSRF_O (Right front ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSRR_I (Right rear ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSRR_O (Right rear ABS pressure reduction solenoid valve output state) | On/Off | • During ABS control: On/Off (solenoid valve is activated/deactivated) • Not ABS control: Off (solenoid valve is deactivated) | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
ABSPMPRLY (Motor relay output state) | On/Off | • Motor relay is activated: On • Motor relay is deactivated: Off | Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | -
ABSVLVRLY (Fail-safe relay output state) | On/Off | • Fail-safe relay is activated: On • Fail-safe relay is deactivated: Off | Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | -
ABS_VOLT (System battery voltage value) | V | • Ignition key at ON: B+ • Idle: Approx. 14-16 V | Inspect power supply circuit. (See DSC HU/CM INSPECTION.) | G
ACCLMTR*1 (Forward-G sensor input) | G | • Vehicle is stopped or driving at a constant speed: 0 G • Cornering to left: Changes between 0 G and 1.5 G • Cornering to right: Changes between 0 G and -1.5 G | Inspect combined sensor. (See COMBINED SENSOR INSPECTION.) | V
AWD_MSG*1 (Missing message from the 4WD control module) | Present/ Not Present | • Present: Circuit in the 4WD control module is normal. • Not Present: Circuit in the 4WD control module is abnormal. | Inspect 4WD control module. (See 4WD CONTROL MODULE INSPECTION [L3 Turbo]) Inspect DSC HU/CM. (See DSC HU/CM INSPECTION) | -
BOO_ABS (Brake pedal switch input) | On/Off | • Brake pedal is depressed: On • Brake pedal is released: Off | Inspect brake switch. (See BRAKE SWITCH INSPECTION.) | -
BRK_FLUID (Brake fluid level sensor input) | OK/Low | • Brake fluid is above LOW: OK • Brake fluid is below LOW: Low | Inspect brake fluid level. Inspect brake fluid level sensor. (See BRAKE FLUID LEVEL SENSOR INSPECTION.) | -
BRAKE_LMP (BRAKE system warning light output state) | On/Off | • BRAKE system warning light is illuminated: On • BRAKE system warning light is not illuminated: Off | Inspect BRAKE system warning light. | -
CCNTABS (Number of continuous codes) | - | DTC is detected: 1-255 DTC is not detected: 0 | Perform inspection using appropriate DTC. | -
IC_MSG (Missing message from the instrument cluster) | Present/ Not Present | • Present: Circuit in the instrument cluster is normal. • Not Present: Circuit in the instrument cluster is abnormal. | Inspect instrument cluster. (See INSTRUMENT CLUSTER INSPECTION) Inspect DSC HU/CM. (See DSC HU/CM INSPECTION) | -
LAT_ACCL (Lateral-G sensor input) | G | • Vehicle is stopped or driving straight: 0 G • Cornering to left: Changes between 0 G and 1.5 G • Cornering to right: Changes between 0 G and -1.5 G | Inspect combined sensor. (See COMBINED SENSOR INSPECTION.) | O
L_DSC_O (Stability control solenoid valve (LF-RR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
LF_WSPD (Left front ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | F, J
LR_WSPD (Left rear ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | N, Q
MCYLI P (Brake fluid pressure sensor input) | Pa | • Brake pedal is released: 0 Pa • Brake pedal is depressed: Changes between 0 Pa and 25.5 MPa | Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | -
PCM_MSG (Missing message from the PCM) | Present/ Not Present | • Present: Circuit in the PCM is normal. • Not Present: Circuit in the PCM is abnormal. | Inspect PCM. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See PCM INSPECTION [MZR-CD (RF Turbo)].) Inspect DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
PMPSTAT (Pump motor output state) | On/Off | • Pump motor activate: On • Pump motor not activate: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
R_DSC_O (Stability control solenoid valve (RF-LR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
RF_WSPD (Right front ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | I, M
RPM (Engine speed signal input) | RPM | • Engine is stopped: 0 RPM • Engine is running: Indicates engine speed | Inspect PCM. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See PCM INSPECTION [MZR-CD (RF Turbo)].) | -
RR_WSPD (Right rear ABS wheel-speed sensor input) | KPH, MPH | • Vehicle is stopped: 0 KPH {0 MPH} • Vehicle is driving: Indicates vehicle speed | Inspect ABS wheel-speed sensor/sensor rotor. (See FRONT/REAR ABS WHEEL-SPEED SENSOR INSPECTION.) | H, K
SWA_POS (Steering angle sensor input) | ° | • Steering wheel is in neutral position: 0 ° • Steering wheel is turned to left: Changes between 0 ° and -1,640 ° • Steering wheel is turned to right: Changes between 0 ° and 1,640 ° | Inspect steering angle sensor. (See STEERING ANGLE SENSOR INSPECTION.) | R, U, W, X
TC LVAL (Traction switch solenoid valve (LF-RR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
TCM_MSG*2 (Missing message from the TCM) | Present/ Not Present | • Present: Circuit in the TCM is normal. • Not Present: Circuit in the TCM is abnormal. | Inspect TCM. (See TCM INSPECTION [FS5A-EL].) (See TCM INSPECTION [JA5AX-EL].) Inspect DSC HU/CM. (See DSC HU/CM INSPECTION.) | -
TC RVAL (Traction switch solenoid valve (RF-LR)) | On/Off | • Solenoid valve is activated: On • Solenoid valve is deactivated: Off | Internal fault of DSC HU/CM. Replace DSC HU/CM. (See DSC HU/CM REMOVAL/INSTALLATION [2WD (MTX), 4WD (ATX)].) (See DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)].) | -
TPI (Throttle position signal input) | % | • Closed throttle position: 0% • Wide open throttle: Changes between 0% and 100% | Inspect PCM and throttle position sensor. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See THROTTLE POSITION (TP) SENSOR INSPECTION [L8, LF, L3].) (See THROTTLE POSITION (TP) SENSOR INSPECTION [L3 Turbo].) | -
TRAC_SW*3 (DSC OFF switch input) | On/Off | • DSC OFF switch is depressed: On • DSC OFF switch is released: Off | Inspect DSC OFF switch. (See DSC OFF SWITCH INSPECTION.) | AA
TRANSGR (Transaxle gear position input) | 1/2/3/4/5/6/R/N/Error | • Transaxle gear /selector lever position*4 1GR: 1 2GR: 2 3GR: 3 4GR: 4 5GR: 5 6GR: 6 Reverse: R Neutral: N When gear position estimation is disabled: Error | Inspect PCM. (See PCM INSPECTION [L8, LF, L3].) (See PCM INSPECTION [L3 Turbo].) (See PCM INSPECTION [MZR-CD (RF Turbo)].) Inspect TCM. (See TCM INSPECTION [FS5A-EL].) (See TCM INSPECTION [JA5AX-EL].) | -
YAW_RATE (Yaw rate sensor input) | °/s | • Vehicle is stopped or driving straight: 0 °/s • Cornering to left: Changes between 0 °/s and 150 °/s • Cornering to right: Changes between 0 °/s and -150 °/s | Inspect combined sensor. (See COMBINED SENSOR INSPECTION.) | T

  *1 :
Only vehicles with 4WD
  *2 :
Only vehicles with ATX
  *3 :
Only vehicles with L3 Turbo
  *4 :
The displayed gear position is an estimated value based on the vehicle wheel speed and engine speed (MTX)

## Active Command Modes Table

Command Name | Definition | Operation | Note
--- | --- | --- | ---
ABS_POWER | Fail-safe relay | On/Off | Ignition key at ON (Engine OFF), and driving
LATACCEL | Lateral-G sensor initialization | TRUE/FALSE
LF_DSC_V | Stability control solenoid valve (LF-RR) | On/Off
LF_INLET | Left front ABS pressure retention solenoid valve | On/Off
LF_OUTLET | Left front ABS pressure reduction solenoid valve | On/Off
LF_TC_VLV | Traction switch solenoid valve (LF-RR) | On/Off
LR_INLET | Left rear ABS pressure retention solenoid valve | On/Off
LR_OUTLET | Left rear ABS pressure reduction solenoid valve | On/Off
PMP_MOTOR | ABS motor | On/Off
RF_DSC_V | Stability control solenoid valve (RF-LR) | On/Off
RF_INLET | Right front ABS pressure retention solenoid valve | On/Off
RF_OUTLET | Right front ABS pressure reduction solenoid valve | On/Off
RF_TC_VLV | Traction switch solenoid valve (RF-LR) | On/Off
RR_INLET | Right rear ABS pressure retention solenoid valve | On/Off
RR_OUTLET | Right rear ABS pressure reduction solenoid valve | On/Off
STAB_IND | DSC indicator light | On/Off
TRAC OFF | DSC OFF light | On/Off
YAWRATE | Yaw rate sensor initialization | On/Off