#
ROOF MOLDING INSTALLATION [WGN]

id0916004476a2

## With Roof Rail

1. Attach the roof molding No.1 to the T stud at the A section.

2. Hook the roof molding No.1 to clip B at the B section, press it in, and attach the roof molding No.1 to clip B.

3. Align the front end-face of roof molding No.2 at a position 216 mm {8.5 in} from the rear end-face of roof molding No.1.

4. Press in roof molding No.2 along the direction (1) shown in the figure and attach it to clips B at the B section.

5. Align the front end-face of roof molding No.3 at a position 47 mm {1.9 in} from the rear end-face of roof molding No.2.

6. Press in roof molding No.3 along the direction (2) shown in the figure and attach it to clips B at the B section.