#
REAR SIDE SEAT BELT REMOVAL/INSTALLATION

id081100804300

  Caution

  • The ELR (emergency locking retractor) has a spring that will unwind if the retractor cover is removed. The spring cannot be rewound by hand. If this occurs, the ELR will not work properly. Therefore, do not disassemble the retractor.

## 4SD

1. Fold the rear seat back.

2. Remove the rear side seats. (See REAR SEAT REMOVAL/INSTALLATION [EXCEPT WGN (4WD)].) (See REAR SEAT REMOVAL/INSTALLATION [WGN (4WD)].)

3. Remove the rear package trim. (See REAR PACKAGE TRIM REMOVAL/INSTALLATION [4SD].)

4. Remove the bolts.

5. Remove the rear seat belt.

6. Install in the reverse order of removal.

## 5HB

  Note

  • Rear side seat belts are built into the rear seat back. See rear seat disassembly/assembly to remove/install the rear side seat belt.

## WGN

  Caution

  • The rear side seat belt for 4WD models is equipped with a silencer to reduse abnormal noise while driving. If the silencer is not installed in the proper position, the push knob may not function properly. When attaching the silencer, be sure to sttach it in the correct area as shown below.

  Note

  • Rear side seat belts are built into the rear seat back. See rear seat disassembly/assembly, to remove/install the rear side seat belt.

1. Peel off the backing of the double-sided adhesive tape.

2. Attach double-sided adhesive tape to the silencer as shown.