BOLT INSPECTION

id011000503300

1. Measure the length of the each bolt.

  • If it exceeds the maximum specification, replace the bolt.

beltze00000026

  Cylinder head bolt length

  Standard
  MZR 2.0 DISI, MZR 2.0 DISI i-stop : 145.2—145.8 mm {5.717—5.740 in}
  MZR 2.3 DISI Turbo : 144.7—145.3 mm {5.697—5.720 in}
  Maximum
  MZR 2.0 DISI, MZR 2.0 DISI i-stop : 146.5 mm {5.767 in}
  MZR 2.3 DISI Turbo : 146 mm {5.748 in}

  Connecting rod bolt length

  Standard
  43.7—44.3 mm {1.720—1.744 in}
  Maximum
  45 mm {1.77 in}