#
DTC B1317, B1318

id080200811500

DTC | B1317 | SAS control module power supply voltage increases (16.1 V or more)
--- | --- | ---
B1318 | SAS control module power supply voltage decreases (less than 9 V)
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • When the SAS control module power supply voltage is not within 9-16 V.
POSSIBLE CAUSE | • Open or short circuit in wiring harness between battery and SAS control module • SAS 10 A fuse malfunction • Battery malfunction • SAS control module malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | INSPECT FUSE • Remove the SAS 10 A fuse. • Is the fuse normal? | Yes | Go to the next step.
No | Replace the fuse.
2 | INSPECT BATTERY • Measure the battery positive voltage. • Is the voltage 9 V-16 V? | Yes | Go to the next step.
No | The battery has a malfunction. Inspect the charge/discharge system.
3 | INSPECT WIRING HARNESS BETWEEN BATTERY AND FUSE BLOCK • Turn the ignition switch to the ON position. • Measure the fuse block terminal N voltage. • Is the voltage 9 V-16 V? | Yes | Install the fuse, then go to the next step.
No | Repair the wiring harness between the fuse block and ignition switch.
4 | INSPECT FUSE BLOCK Warning • Handling the air bag system components improperly can accidentally deploy the air bag modules and pre-tensioner seat belts, which may seriously injure you. Read the service warnings and cautions before handling the air bag system components. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.) • Turn the ignition switch to the LOCK position. • Disconnect the negative battery cable and wait for 1 min or more. • Remove the column cover. (See COLUMN COVER REMOVAL/INSTALLATION.) • Disconnect the clock spring connector. • Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.) • Disconnect the passenger-side air bag module connector. • Disconnect the driver and passenger-side curtain air bag module connector. • Disconnect the front seat connector. • Remove the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.) • Disconnect the SAS control module connector. • Turn the ignition switch to the ON position. • Measure the SAS control module terminal 1W voltage. • Is the voltage 9 V-16 V? | Yes | Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)
No | Repair the wiring harness between the fuse block and SAS control module.