#
POWER OUTSIDE MIRROR DISASSEMBLY/ASSEMBLY [TYPE B]

id0912008075b4

## Mirror Glass Removal

1. Press area A of the mirror glass so that area B moves outward.

2. Disengage clip A while lifting up the inside of the mirror glass holder.

3. Pull the mirror glass holder outward, then disengage clips B by pulling them out.

4. Remove the mirror glass holder and the mirror glass as a single unit.

## Mirror Garnish Removal

1. Remove the mirror glass from the outside mirror. (See Mirror Glass Removal.)

2. Pinch the clip ends using pincers and detach the clips by pushing them forward.

3. Grasp the upper side of the mirror garnish and remove it by pulling it in the direction of the arrow.

## Mirror Garnish Installation

1. Position the mirror garnish against the mirror body in the direction of the arrow shown in the figure, and insert the mirror garnish clips (6 locations) into the mirror body.

2. Install the mirror garnish so that there are no gaps around the component.

## Mirror Glass Installation

1. Press the mirror glass at clip A and engage it to the frame.

2. Engage clips B while pushing the mirror glass to the frame.