#
FRONT FENDER PANEL REMOVAL/INSTALLATION

id091000405900

1. Disconnect the negative battery cable.

2. Remove the front side turn light.

3. Remove the fender molding. (See COWL GRILLE REMOVAL/INSTALLATION.)

4. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

5. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

1 | Front fender panel
2 | Seal plate

7. Install in the reverse order of removal.