#
CAR-NAVIGATION UNIT STRUCTURAL VIEW

id092000108500
• The car-navigation unit is located in the glove compartment.
• An Eject button, to eject the DVD-ROM from the loading slot, is included in the unit.
• A gyro sensor which detects vehicle cornering angle is built into the unit.

.

1 | DVD-ROM loading slot
2 | DVD-ROM
3 | Eject button

## Terminal Layout and Signals

Terminal | Signals
--- | ---
16-pin connector
| 1A | GND
1B | B+
1C | -
1D | ACC
1E | -
1F | -
1G | -
1H | Vehicle speed
1I | -
1J | -
1K | -
1L | R-range
1M | Front speaker output (-)
1N | Front speaker output (+)
1O | Front speaker input (-)
1P | Front speaker input (+)

Terminal | Signals
--- | ---
24-pin connector
| 2A | -
2B | -
2C | -
2D | -
2E | -
2F | -
2G | -
2H | -
2I | -
2J | -
2K | -
2L | -
2M | -
2N | Monitor serial input
2O | Shield GND
2P | Monitor serial output
2Q | Shield GND
2R | Video (composit sync)
2S | -
2T | Video (B)
2U | Video GND
2V | Video (G)
2W | -
2X | Video (R)

Terminal | Signals
--- | ---
6-pin connector
| 3A | Mic (+)
3B | Mic (-)
3C | Mic power
3D | GND
3E | Mic sense
3F | -

Terminal | Signal
--- | ---
1-pin connector
| 4A | GPS antenna input

Terminal | Signal
--- | ---
1-pin connector
| 5A | RDS-TMC antenna input

Terminal | Signal
--- | ---
1-pin connector
| 6A | GND