#
FRONT DOOR GLASS REMOVAL/INSTALLATION

id091200415600

1. Operate the front door glass so that the distance from the top of the front door glass to the upper part of the rear beltline molding is 210 mm {8.3 in}.

2. Disconnect the negative battery cable.

3. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the hole cover.

5. Remove the screws.

6. Insert your hand in hole of the front door unit, and lift out the front door glass.

7. Install in the reverse order of removal.