#
MAIN FUSE REMOVAL/INSTALLATION

id092100801500

1. Disconnect the negative battery cable.

2. Remove the Battery. (See BATTERY REMOVAL/INSTALLATION [L8, LF, L3, L3 Turbo].) (See BATTERY REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the Air cleaner cover and Air cleaner case. (See INTAKE AIR SYSTEM REMOVAL/INSTALLATION [L8, LF, L3].)

4. Remove the main fuse block cover.

5. Remove in the order indicated in the table.

1 | Nut
2 | Bolt (See Bolt Removal Note.)
3 | Main fuse

6. Install in the reverse order of removal.

## Bolt Removal Note

1. Press and remove the tabs on the main fuse block at the positions indicated by the arrows.

2. Press the tabs in the position indicated by the arrows in the figure to separate the main fuse into two.

3. Lift up the main fuse block and remove the bolts.