#
DTC P0606 [MZR-CD (RF Turbo)]

id0102f1809400

DTC P0606 | PCM malfunction
--- | ---
DETECTION CONDITION | • PCM internal malfunction. Diagnostic support note • The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle. • FREEZE FRAME DATA is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | - | - | Replace the PCM. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)