#
INTAKE AIR TEMPERATURE (IAT) SENSOR CONSTRUCTION/OPERATION [MZR-CD (RF Turbo)]

id0140f1173600
• Installed to the air cleaner.
• Built into the mass airflow sensor.

1 | IAT sensor
2 | MAF sensor

• The thermistor type IAT sensor changes resistance according to the IAT.
• The resistance decreases if the IAT increases and, conversely, increases if the IAT decreases.

1 | IAT sensor
2 | IAT sensor characteristic
3 | Resistance
4 | Large
5 | Small
6 | High
7 | Low