#
DTC P0708 [FS5A-EL]

id050221801100

DTC P0708 | Transaxle range (TR) switch circuit high input
--- | ---
DETECTION CONDITION | • When all conditions below are satisfied and 100 s or more have passed. - Vehicle speed 20 km/h {12 mph} or more - Engine speed 530 rpm or more - Voltage at TCM terminal 2H 4.79 V or more Diagnostic support note: • This is a continuous monitor (CCM). • The MIL illuminates if the TCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the TCM. • The PENDING CODE is available if the TCM detects the above malfunction condition during the first drive cycle. • FREEZE FRAME DATA is available. • The AT warning light illuminates. • The DTC is stored in the TCM memory.
POSSIBLE CAUSE | • TR switch malfunction • Open circuit in wiring harness between TR switch terminal C and TCM terminal 2H • Short to power supply in wiring harness between TR switch terminal C and TCM terminal 2H • Open circuit in wiring harness between TR switch terminal B and TCM terminal 2O • Poor connection of TR switch or TCM connectors • TCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has the FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Bulletins and/or on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT TR SWITCH CONNECTOR FOR POOR CONNECTION • Turn the ignition switch to the LOCK position. • Disconnect the TR switch connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Are TR switch terminals normal? | Yes | Go to the next step.
No | Repair terminals or replace the TR switch, then go to Step 9. (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [FS5A-EL].)
4 | INSPECT TR SWITCH • Inspect for resistance between TR switch terminals B and C (part-side). • Is the resistance normal? (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FS5A-EL].) | Yes | Go to the next step.
No | Replace the TR switch, then go to Step 9. (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [FS5A-EL].)
5 | INSPECT TCM CONNECTOR FOR POOR CONNECTION • Disconnect the TCM connector. • Inspect for poor connection at terminals 2H and 2O (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the terminal, then go to step 9.
No | Go to the next step.
6 | INSPECT TR SWITCH SIGNAL CIRCUIT FOR SHORT TO POWER SUPPLY • Turn the ignition switch to the ON position (engine off). • Inspect the voltage between TR switch terminal C and (wiring harness-side) body ground. • Is the voltage B+? | Yes | Repair or replace the wiring harness for short to power supply, then go to Step 9.
No | Go to the next step.
7 | INSPECT TR SWITCH SIGNAL CIRCUIT FOR OPEN CIRCUIT • Inspect for continuity between TR switch terminal C (wiring harness-side) and TCM terminal 2H. • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for open circuit, then go to step 9.
8 | INSPECT TR SWITCH GROUND CIRCUIT FOR OPEN CIRCUIT • Inspect for continuity between TR switch terminal B (wiring harness-side) and TCM terminal 2O. • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0708 COMPLETED • Make sure to reconnect all the disconnected connectors. • Clear the DTC from the memory using the WDS or equivalent. • Drive the vehicle for 100 s or more under the following conditions: - Engine speed (RPM PID) 530 rpm or more - Vehicle speed (VSS PID) 20 km/h {12 mph} or more • Is the PENDING CODE present? | Yes | Replace the TCM, then go to the next step. (See TCM REMOVAL/INSTALLATION [FS5A-EL].)
No | No concern is detected. Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [FS5A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection.
No | DTC troubleshooting completed.