#
FUEL PRESSURE CONTROL OUTLINE [MZR-CD (RF Turbo)]

id0140f1186300
• The PCM performs the feedback control of the fuel pressure in the common rail to gain optimum fuel injection pressure according to engine operation conditions.
• Because the fuel pressure can be controlled regardless of engine operation conditions, high pressure fuel injection even with low engine speed is possible. Due to this, generation of NOx and particulate matter can be reduced.