#
REFRIGERANT PRESSURE SWITCH INSPECTION

id074000802700

1. Install the SST (49 C061 0A0B).

2. Disconnect the refrigerant pressure switch connector.

3. Verify the high-pressure side reading of the SST (49 C061 001A) and continuity between the terminals of the refrigerant pressure switch.

  • If not as specified, replace the refrigerant pressure switch.

## Triple-pressure Type

## Dual-pressure Type