#
DIFFERENTIAL OIL TEMPERATURE SENSOR REMOVAL/INSTALLATION [L3]

id0318a1805700

  Warning

  • Hot differential oil may cause severe burns. Do not perform maintenance while differential oil is hot.

1. Disconnect the negative (-) battery cable.

2. Disconnect the differential oil temperature sensor connector.

3. Remove the differential oil temperature sensor.

4. Apply differential oil to the O-ring.

5. Install the differential oil temperature sensor.

Tightening torque

  12.7-17.3 N·m {1.3-1.7 kgf·m, 9.4-12.7 ft·lbf}

6. Connect the differential oil temperature sensor connector.

7. Connect the negative (-) battery cable.