#
REAR CENTER SEAT BELT REMOVAL/INSTALLATION

id081100800900

  Caution

  • The ELR (emergency locking retractor) has a spring that will unwind if the retractor cover is removed. The spring cannot be rewound by hand. If this occurs, the ELR will not work properly. Therefore, do not disassemble the retractor.

## 4SD

1. Fold the rear seat back.

2. Remove the rear package trim (See REAR PACKAGE TRIM REMOVAL/INSTALLATION [4SD].)

3. Remove the bolt.

4. Remove the rear center seat belt.

5. Install in the reverse order of removal.

## 5HB

1. Remove the following parts:

  (1) Rear scuff plate (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)
  (2) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (3) Trunk side upper trim (See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [5HB].)
  (4) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB].)

2. Remove the bolts.

3. Remove the rear center seat belt.

4. Install in the reverse order of removal.

## WGN

1. Remove the headliner. (See HEADLINER REMOVAL/INSTALLATION [WGN].)

2. Remove the bolts.

3. Remove the rear center seat belt.

4. Install in the reverse order of removal.