DTC C1119 [ABS/TCS]

id040214874000

DTC | C1119 | Engine control system, torque reduction inhibit signal line
DETECTION CONDITION | • Engine RPM information through CAN is out of specification or invalid value. • Throttle information through CAN is out of specification or invalid value. • Received control prohibition signal from PCM through CAN.
POSSIBLE CAUSE | • Malfunction of PCM

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT FOR PCM FOR DTCs • Turn the ignition switch off. • Connect WDS or equivalent to DLC-2 • Turn ignition key to ON (engine off). • Is DTC for engine control system obtained? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [L8, LF, L3].) (See DTC TABLE [L3 Turbo].) (See DTC TABLE [MZR-CD (RF Turbo)].)
No | Go to the next step.
2 | VERIFY TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the memory. (See DTC Table • Start engine.) • Is same DTC present? | Yes | Replace ABS (ABS/TCS) HU/CM, then go to the next step.
No | Go to the next step.
3 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | Troubleshooting completed.