#
AUTOMATIC TRANSAXLE SPECIFICATIONS

D6E051700000A06

Item | Specification
--- | ---
Engine type | LF | L3
Automatic transaxle type | FS5A-EL
Gear ratio | 1GR | 3.620
2GR | 1.925
3GR | 1.285
4GR | 0.939
5GR | 0.692
Reverse | 3.405
Final gear ratio | 3.863
ATF | Type | ATF M-V
Capacity (Approx. quantity) | (L {US qt, lmp qt}) | 8.14 {8.60, 7.16}
Torque converter stall torque ratio | 2.07 | 1.84
Hydraulic system (Number of drive/driven gear plates) | Forward clutch | 4/4
3-4 clutch | 3/3
Reverse clutch | 2/2
Direct clutch | 2/3
Low and reverse brake | 5/5
Reduction brake | 3/5
Band servo | Servo diameter (Piston outer dia.) | (mm {in}) | 64.6 {2.54}
Front planetary gear (Number of teeth) | Front sun gear | 49
Front pinion gear | 20
Front internal gear | 89
Rear planetary gear (Number of teeth) | Rear sun gear | 37
Rear pinion gear | 30
Rear internal gear | 98
Primary gear (number of teeth) | 86
Secondary gear (number of teeth) | 82
Secondary planetary gear (Number of teeth) | Secondary sun gear | 31
Secondary pinion gear | 29
Secondary internal gear | 89
Output gear (number of teeth) | 22
Ring gear (number of teeth) | 85