DTC TABLE [MZR-CD (RF Turbo)]

id0102f1545200

×: Applicable —: Not applicable

DTC | Condition | MIL | DC | Self-test type*1 | Memory function | Page
--- | --- | --- | --- | --- | --- | ---
B1213 | Number of valid keys is below minimum | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
B1342 | ECU is faulted | (See DTC TABLE [BCM])
B1600 | ID number signal is not received | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
B1601 | • PCM received incorrect ID number from key (transponder) • Keyless control module malfunction*2 | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
B1602 | PCM received invalid format of ID number from transponder | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
B1681 | • Communication error between the keyless control module and the coil antenna*2 • Communication error between the keyless control module and the PCM*2 • Coil signal is not received*3 | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
B1681 | Communication error between the keyless control module and the PCM | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
B2103 | Coil Antenna failure | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
B2431 | • ID number signal is not received*2 • Transponder programming failure*3 | (See DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS SYSTEM)]) (See DTC TABLE [IMMOBILIZER SYSTEM (KEYLESS ENTRY SYSTEM)])
P0016 | CKP-CMP correlation | ON | 2 | C | × | (See DTC P0016 [MZR-CD (RF Turbo)])
P0030 | A/F sensor heater control circuit problem | ON | 2 | C | × | (See DTC P0030 [MZR-CD (RF Turbo)])
P0045 | Variable boost control (VBC) solenoid valve control circuit low or high input | ON | 1 | C/R | × | (See DTC P0045 [MZR-CD (RF Turbo)])
P0071 | Exhaust gas pressure correction temperature sensor circuit range/performance malfunction | — | — | C | — | (See DTC P0071 [MZR-CD (RF Turbo)])
P0072 | Exhaust gas pressure correction temperature sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P0072 [MZR-CD (RF Turbo)])
P0073 | Exhaust gas pressure correction temperature sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P0073 [MZR-CD (RF Turbo)])
P0088 | Fuel pressure system too high | ON | 2 | C/R | × | (See DTC P0088 [MZR-CD (RF Turbo)])
P0089 | Fuel pressure regulator performance | — | — | C/R | — | (See DTC P0089 [MZR-CD (RF Turbo)])
P0093 | Fuel system leak detection | ON | 1 | C/R | × | (See DTC P0093 [MZR-CD (RF Turbo)])
P0096 | Intake air temperature (IAT) sensor No.2 circuit range/performance malfunction | ON | 2 | C | × | (See DTC P0096 [MZR-CD (RF Turbo)])
P0097 | Intake air temperature (IAT) sensor No.2 circuit low input | ON | 1 | C/O/R | × | (See DTC P0097 [MZR-CD (RF Turbo)])
P0098 | Intake air temperature (IAT) sensor No.2 circuit high input | ON | 1 | C/O/R | × | (See DTC P0098 [MZR-CD (RF Turbo)])
P0101 | Mass airflow (MAF) sensor range/performance malfunction | ON | 1 | C | × | (See DTC P0101 [MZR-CD (RF Turbo)])
P0102 | Mass airflow (MAF) sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P0102 [MZR-CD (RF Turbo)])
P0103 | Mass airflow (MAF) sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P0103 [MZR-CD (RF Turbo)])
P0104 | Mass airflow (MAF) sensor circuit malfunction | — | — | C | — | (See DTC P0104 [MZR-CD (RF Turbo)])
P0106 | Boost sensor range/performance malfunction | ON | 1 | C | × | (See DTC P0106 [MZR-CD (RF Turbo)])
P0107 | Boost sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P0107 [MZR-CD (RF Turbo)])
P0108 | Boost sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P0108 [MZR-CD (RF Turbo)])
P0111 | Intake air temperature (IAT) sensor No.1 range/performance malfunction | ON | 2 | C | × | (See DTC P0111 [MZR-CD (RF Turbo)])
P0112 | Intake air temperature (IAT) sensor No.1 circuit low input | ON | 1 | C/O/R | × | (See DTC P0112 [MZR-CD (RF Turbo)])
P0113 | Intake air temperature (IAT) sensor No.1 circuit high input | ON | 1 | C/O/R | × | (See DTC P0113 [MZR-CD (RF Turbo)])
P0116 | Engine coolant temperature (ECT) sensor range/performance malfunction | ON | 2 | C | × | (See DTC P0116 [MZR-CD (RF Turbo)])
P0117 | Engine coolant temperature (ECT) sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P0117 [MZR-CD (RF Turbo)])
P0118 | Engine coolant temperature (ECT) sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P0118 [MZR-CD (RF Turbo)])
P0121 | Accelerator pedal position (APP) sensor No.1/No.2 position correlation | ON | 1 | C | × | (See DTC P0121 [MZR-CD (RF Turbo)])
P0122 | Accelerator pedal position (APP) sensor No.1 circuit low input | ON | 1 | C/O/R | × | (See DTC P0122 [MZR-CD (RF Turbo)])
P0123 | Accelerator pedal position (APP) sensor No.1 circuit high input | ON | 1 | C/O/R | × | (See DTC P0123 [MZR-CD (RF Turbo)])
P0131 | A/F sensor circuit low input | ON | 1 | C | × | (See DTC P0131 [MZR-CD (RF Turbo)])
P0132 | A/F sensor circuit high input | ON | 1 | C | × | (See DTC P0132 [MZR-CD (RF Turbo)])
P0133 | A/F sensor circuit malfunction | ON | 2 | C | × | (See DTC P0133 [MZR-CD (RF Turbo)])
P0134 | A/F sensor no activity detected | ON | 2 | C/R | × | (See DTC P0134 [MZR-CD (RF Turbo)])
P0140 | A/F sensor no activity | — | — | C | — | (See DTC P0140 [MZR-CD (RF Turbo)])
P0151 | A/F sensor circuit low input | ON | 1 | C | × | (See DTC P0151 [MZR-CD (RF Turbo)])
P0152 | A/F sensor circuit high input | ON | 1 | C | × | (See DTC P0152 [MZR-CD (RF Turbo)])
P0154 | A/F sensor circuit no activity detected | ON | 1 | C | × | (See DTC P0154 [MZR-CD (RF Turbo)])
P0181 | Fuel temperature sensor circuit range/performance malfunction | — | — | C | — | (See DTC P0181 [MZR-CD (RF Turbo)])
P0182 | Fuel temperature sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P0182 [MZR-CD (RF Turbo)])
P0183 | Fuel temperature sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P0183 [MZR-CD (RF Turbo)])
P0191 | Fuel pressure sensor range/performance malfunction | ON | 2 | C | × | (See DTC P0191 [MZR-CD (RF Turbo)])
P0192 | Fuel pressure sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P0192 [MZR-CD (RF Turbo)])
P0193 | Fuel pressure sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P0193 [MZR-CD (RF Turbo)])
P0201 | Fuel injector No.1 operation identified | ON | 1 | C/R | × | (See DTC P0201 [MZR-CD (RF Turbo)])
P0202 | Fuel injector No.2 operation identified | ON | 1 | C/R | × | (See DTC P0202 [MZR-CD (RF Turbo)])
P0203 | Fuel injector No.3 operation identified | ON | 1 | C/R | × | (See DTC P0203 [MZR-CD (RF Turbo)])
P0204 | Fuel injector No.4 operation identified | ON | 1 | C/R | × | (See DTC P0204 [MZR-CD (RF Turbo)])
P0219 | Engine overspeed condition | — | — | C | — | (See DTC P0219 [MZR-CD (RF Turbo)])
P0222 | Accelerator pedal position (APP) sensor No.2 circuit low input | ON | 1 | C/O/R | × | (See DTC P0222 [MZR-CD (RF Turbo)])
P0223 | Accelerator pedal position (APP) sensor No.2 circuit high input | ON | 1 | C/O/R | × | (See DTC P0223 [MZR-CD (RF Turbo)])
P0234 | Turbocharger overboost condition | — | — | C | — | (See DTC P0234 [MZR-CD (RF Turbo)])
P0299 | Turbocharger underboost condition | — | — | C | — | (See DTC P0299 [MZR-CD (RF Turbo)])
P0301 | Cylinder No.1 misfire detection | ON | 2 | C/R | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0302 | Cylinder No.2 misfire detection | ON | 2 | C/R | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0303 | Cylinder No.3 misfire detection | ON | 2 | C/R | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0304 | Cylinder No.4 misfire detection | ON | 2 | C/R | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0336 | CKP sensor range/performance malfunction | ON | 2 | C | × | (See DTC P0336 [MZR-CD (RF Turbo)])
P0337 | CKP sensor circuit low input | ON | 1 | C | × | (See DTC P0337 [MZR-CD (RF Turbo)])
P0341 | CMP sensor range/performance malfunction | ON | 2 | C | × | (See DTC P0341 [MZR-CD (RF Turbo)])
P0342 | CMP sensor circuit low input | ON | 1 | C | × | (See DTC P0342 [MZR-CD (RF Turbo)])
P0400 | EGR flow problem | ON | 2 | C/R | × | (See DTC P0400 [MZR-CD (RF Turbo)])
P0401 | EGR flow insufficient detected | ON | 2 | C | × | (See DTC P0401 [MZR-CD (RF Turbo)])
P0402 | EGR flow excessive detected | ON | 2 | C | × | (See DTC P0402 [MZR-CD (RF Turbo)])
P0403 | EGR control circuit | ON | 2 | C/O/R | × | (See DTC P0403 [MZR-CD (RF Turbo)])
P0404 | EGR control circuit range/performance | ON | 2 | C/O/R | × | (See DTC P0404 [MZR-CD (RF Turbo)])
P0405 | EGR sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P0405 [MZR-CD (RF Turbo)])
P0406 | EGR valve position sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P0406 [MZR-CD (RF Turbo)])
P0500 | VSS circuit malfunction | ON | 1 | C | × | (See DTC P0500 [MZR-CD (RF Turbo)])
P0504 | Brake switch circuit problem | — | — | C | — | (See DTC P0504 [MZR-CD (RF Turbo)])
P0512 | Engine switch circuit high input | ON | 1 | C | × | (See DTC P0512 [MZR-CD (RF Turbo)])
P0545 | Exhaust gas temperature sensor (upper) circuit low input | ON | 1 | C/O/R | × | (See DTC P0545 [MZR-CD (RF Turbo)])
P0546 | Exhaust gas temperature sensor (upper) circuit high input | ON | 1 | C/R | × | (See DTC P0546 [MZR-CD (RF Turbo)])
P0548 | Exhaust gas temperature sensor (middle) circuit low input | ON | 1 | C/O/R | × | (See DTC P0548 [MZR-CD (RF Turbo)])
P0549 | Exhaust gas temperature sensor (middle) circuit high input | ON | 1 | C/R | × | (See DTC P0549 [MZR-CD (RF Turbo)])
P0562 | Battery voltage low input | ON | 1 | C | × | (See DTC P0562 [MZR-CD (RF Turbo)])
P0563 | Battery voltage high input | ON | 1 | C | × | (See DTC P0563 [MZR-CD (RF Turbo)])
P0564 | Cruise control switch circuit malfunction | — | — | C | — | (See DTC P0564 [MZR-CD (RF Turbo)])
P0601 | Internal control module memory check sum error | ON | 1 | C/O/R | × | (See DTC P0601 [MZR-CD (RF Turbo)])
P0602 | PCM programming error | ON | 1 | C/O/R | × | (See DTC P0602 [MZR-CD (RF Turbo)])
P0605 | PCM memory check sum error | ON | 1 | C/O/R | × | (See DTC P0605 [MZR-CD (RF Turbo)])
P0606 | PCM malfunction | ON | 1 | C/O/R | × | (See DTC P0606 [MZR-CD (RF Turbo)])
P0607 | PCM performance problem | — | — | C/O/R | — | (See DTC P0607 [MZR-CD (RF Turbo)])
P0610 | PCM vehicle options error | ON | 1 | C/O/R | × | (See DTC P0610 [MZR-CD (RF Turbo)])
P0628 | Suction control valve circuit low input | ON | 1 | C/R | × | (See DTC P0628 [MZR-CD (RF Turbo)])
P0629 | Suction control valve circuit high input | ON | 1 | C/R | × | (See DTC P0629 [MZR-CD (RF Turbo)])
P0704 | Clutch switch circuit malfunction | ON | 2 | C | × | (See DTC P0704 [MZR-CD (RF Turbo)])
P0850 | Neutral switch circuit malfunction | ON | 2 | C | × | (See DTC P0850 [MZR-CD (RF Turbo)])
P1196 | Key off voltage high | — | — | C | — | (See DTC P1196 [MZR-CD (RF Turbo)])
P1211 | Common rail pressure higher/lower than desired (engine running) | ON | 2 | C/R | × | (See DTC P1211 [MZR-CD (RF Turbo)])
P1281 | Common rail pressure higher than desired (engine running) | ON | 2 | C/R | × | (See DTC P1281 [MZR-CD (RF Turbo)])
P1303 | EGR calibration fault | ON | 2 | C | × | (See DTC P1303 [MZR-CD (RF Turbo)])
P1329 | Common rail pressure higher than desired (engine running) | ON | 2 | C | × | (See DTC P1329 [MZR-CD (RF Turbo)])
P1378 | Fuel injector supply voltages circuit low input | ON | 1 | C/R | × | (See DTC P1378 [MZR-CD (RF Turbo)])
P1379 | Fuel injector supply voltages circuit high input | ON | 1 | C/R | × | (See DTC P1379 [MZR-CD (RF Turbo)])
P1391 | Glow plug circuit low input | — | — | C/O | — | (See DTC P1391 [MZR-CD (RF Turbo)])
P1392 | Glow plug circuit high input | — | — | C | — | (See DTC P1392 [MZR-CD (RF Turbo)])
P1588 | Intake shutter valve construction problem | ON | 2 | C | × | (See DTC P1588 [MZR-CD (RF Turbo)])
P1589 | Intake shutter valve control range/performance | ON | 1 | C/R | × | (See DTC P1589 [MZR-CD (RF Turbo)])
P1675 | Injector data not programmed | ON | 1 | C/O/R | × | (See DTC P1675 [MZR-CD (RF Turbo)])
P1676 | Checksum corrupt | ON | 1 | C/O/R | × | (See DTC P1676 [MZR-CD (RF Turbo)])
P2002 | Diesel particulate filter efficiency less than threshold | ON | 2 | C | × | (See DTC P2002 [MZR-CD (RF Turbo)])
P2032 | Exhaust gas temperature sensor (lower) circuit low input | ON | 1 | C/O/R | × | (See DTC P2032 [MZR-CD (RF Turbo)])
P2033 | Exhaust gas temperature sensor (lower) circuit high input | ON | 1 | C/R | × | (See DTC P2033 [MZR-CD (RF Turbo)])
P2101 | Intake shutter valve position sensor circuit high input | ON | 2 | C/R | × | (See DTC P2101 [MZR-CD (RF Turbo)])
P2105 | Intake shutter valve actuator control system-forced engine shutdown | — | — | C | — | (See DTC P2105 [MZR-CD (RF Turbo)])
P2135 | Accelerator pedal position (APP) sensor No.1/No.2 voltage correlation | ON | 1 | C/R | × | (See DTC P2135 [MZR-CD (RF Turbo)])
P2146 | Fuel injector No.1 and No.3 operation identified | ON | 1 | C/R | × | (See DTC P2146 [MZR-CD (RF Turbo)])
P2147 | Fuel injector supply circuit low input | ON | 1 | C/R | × | (See DTC P2147 [MZR-CD (RF Turbo)])
P2148 | Fuel injector supply voltages circuit high input | ON | 1 | C/R | × | (See DTC P2148 [MZR-CD (RF Turbo)])
P2149 | Fuel injector No.2 and No.4 operation identified | ON | 1 | C/R | × | (See DTC P2149 [MZR-CD (RF Turbo)])
P2227 | BARO sensor range/performance malfunction | ON | 2 | C | × | (See DTC P2227 [MZR-CD (RF Turbo)])
P2228 | BARO sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P2228 [MZR-CD (RF Turbo)])
P2229 | BARO sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P2229 [MZR-CD (RF Turbo)])
P242F | Diesel particulate filter restriction-soot accumulation | ON | 1 | C | × | (See DTC P242F [MZR-CD (RF Turbo)])
P2428 | Exhaust gas temperature too high | — | — | C | — | (See DTC P2428 [MZR-CD (RF Turbo)])
P2452 | Exhaust gas pressure sensor circuit problem | — | — | C | — | (See DTC P2452 [MZR-CD (RF Turbo)])
P2453 | Exhaust gas pressure sensor circuit range/performance malfunction | — | — | C | — | (See DTC P2453 [MZR-CD (RF Turbo)])
P2454 | Exhaust gas pressure sensor circuit low input | ON | 1 | C/O/R | × | (See DTC P2454 [MZR-CD (RF Turbo)])
P2455 | Exhaust gas pressure sensor circuit high input | ON | 1 | C/O/R | × | (See DTC P2455 [MZR-CD (RF Turbo)])
P2456 | Exhaust gas pressure sensor circuit intermittent/erratic | — | — | C | — | (See DTC P2456 [MZR-CD (RF Turbo)])
P2458 | Diesel particulate filter regeneration duration | — | — | C | — | (See DTC P2458 [MZR-CD (RF Turbo)])
P2459 | Diesel particulate filter regeneration frequency | — | — | C | — | (See DTC P2459 [MZR-CD (RF Turbo)])
P252F | Engine oil level too high | — | — | C | — | (See DTC P252F [MZR-CD (RF Turbo)])
P253F | Engine oil deteriorated | — | — | C | — | (See DTC P253F [MZR-CD (RF Turbo)])
P2621 | Intake shutter valve position sensor circuit low output | ON | 1 | C/O/R | × | (See DTC P2621 [MZR-CD (RF Turbo)])
P2622 | Intake shutter valve position sensor circuit high output | ON | 1 | C/O/R | × | (See DTC P2622 [MZR-CD (RF Turbo)])
U0073 | CAN system communication error | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0121 | Communication error to DSC HU/CM or ABS HU/CM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0155 | Communication error to instrument cluster | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0166 | Communication error to water heater unit | — | — | C | × | (See DTC U0166 [MZR-CD (RF Turbo)])

*1 :C; CMDTC self test, O; KOEO self test, R; KOER self test
*2 :With advanced keyless system
*3 :Without advanced keyless system