#
SUNROOF MOTOR INSPECTION

id091500801100

## Motor

1. Apply battery positive voltage to the sunroof motor terminals and inspect the operation of the sunroof motor.

  • If not as specified, replace the sunroof motor.

Connection | Motor operation
--- | ---
2A | 2B
B+ | GND | Turn left (Slide close/Tilt up)
GND | B+ | Turn right (Slide open/Tilt down)

## Limit Switch

1. Inspect for continuity between the sunroof motor terminals using an ohmmeter.

  • If not as specified, replace the sunroof motor.