#
GENERATOR DISASSEMBLY/ASSEMBLY [L8, LF, L3]

id0117b18004a9

  Caution

  • Melt the solder quickly, otherwise the diodes (rectifier) and regulator will be damaged by excessive heat.

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Front cover
2 | Pulley
3 | Rotor
4 | Bearing
5 | Generator heat insulator
6 | Stator coil
7 | Rectifier
8 | Brush holder
9 | Rear bracket