#
FUEL SYSTEM OUTLINE

id0114b1100100

## Features

Improved serviceability | • Nylon tubes adopted for fuel hoses in the engine compartment and around the fuel tank, and quick release connectors adopted for joints
Reduction of evaporative gas | • Returnless fuel system adopted

## Specification

Item | Specification
--- | ---
Injector | Type | Hi-ohmic
Type of fuel delivery | Top-feed
Type of drive | Voltage
Pressure regulator control pressure | (kPa {kgf/cm2, psi}) | Approx. 380 {3.87, 55.1}
Fuel pump type | Electric
Fuel tank capacity | (L {US gal, lmp gal}) | 64 {16.9, 14.1}*1, 62 {16.4, 13.6}*2

  *1 :
2WD
  *2 :
4WD

Fuel type

Fuel | Research octane number | Country
Premium unleaded fuel (Conforming to EN 228*1) (Conforming to Fuel Quality Standards Act 2000*2) | 95 or above | European countries, Kuwait, Saudi Arabia, UAE, Bahrain, Qatar, Oman, Chile, Taiwan, Hong Kong, Brunei, Macao, Singapore, Lebanon*3, Costa Rica*3, Guatemala*3, Panama*3, El Salvador*3, Dominican Republic*3, Curacao*3, The Philippines*3, South Africa*3, Trinidad and Tobago*3, Barbados*3, Jamaica*3, Australia*3, New Zealand*3, Fiji*3, Malaysia*3, Thailand*3, Indonesia*3
Regular unleaded fuel (Conforming to Fuel Quality Standards Act 2000*2) | 91 | Peru
90 or above | Virgin Islands, St. Martin, Aruba, Haiti, Palau, Micronesia, Algeria, Syria, Marshall Islands, Vanuatu, Samoa, Nigeria, Madagascar, Tunisia, Jordan, Paraguay, Tahiti, Honduras, Nicaragua, Bolivia, Papua New Guinea, Nepal, Antigua, St. Lucia, The Commonwealth of Dominica, Suriname, Lebanon*4, Dominican Republic*4, Curacao*4, Panama*4, El Salvador*4, Costa Rica*4, Guatemala*4, South Africa*4, Trinidad and Tobago*4, Fiji*4, Barbados*4, Jamaica*4, The Philippines*4, Australia*4, New Zealand*4, Malaysia*4

  *1 :
Europe
  *2 :
Australia
  *3 :
L3
  *4 :
LF