#
SUSPENSION TECHNICAL DATA

id025000800100

## Front Suspension (Unloaded)

• Unloaded: Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.

4SD, 5HB

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Maximum steering angle | Inner | 18 inch wheel specification vehicles: 36°±3° Except for above: 39°±3°
Outer | 18 inch wheel specification vehicles: 30°±3° Except for above: 31°±3°
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Caster angle*1 (Reference value) | normal | 3°37'±1° | 3°39'±1° | 3°41'±1° | 3°44'±1° | 3°47'±1°
elevated*2 | 3°32'±1° | 3°34'±1° | 3°36'±1° | 3°39'±1° | 3°42'±1°
Camber angle*1 (Reference value) | normal | -0°16'±1° | -0°17'±1°
elevated*2 | -0°09'±1° | -0°10'±1°
Steering axis inclination (Reference value) | normal | 5°26' | 5°28'
elevated*2 | 5°17' | 5°18'

  *1 :
Difference between left and right must not exceed 1°30'.
  *2 :
Distance between wheel center and fender brim is 402 mm {15.8 in} (reference value).

WGN 2WD

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Maximum steering angle | Inner | 18 inch wheel specification vehicles: 36°±3° Except for above: 39°±3°
Outer | 18 inch wheel specification vehicles: 30°±3° Except for above: 31°±3°
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Caster angle*1 (Reference value) | normal | 3°30'±1° | 3°32'±1° | 3°34'±1° | 3°37'±1° | 3°40'±1°
elevated*2 | 3°25'±1° | 3°27'±1° | 3°29'±1° | 3°32'±1° | 3°35'±1°
Camber angle*1 (Reference value) | normal | -0°14'±1° | -0°15'±1°
elevated*2 | -0°07'±1° | -0°08'±1°
Steering axis inclination (Reference value) | normal | 5°24'
elevated*2 | 5°15' | 5°16'

  *1 :
Difference between left and right must not exceed 1°30'.
  *2 :
Distance between wheel center and fender brim is 405 mm {15.94 in} (reference value).

WGN 4WD

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Maximum steering angle | Inner | 39°±3°
Outer | 31°±3°
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Caster angle*1 (reference value) | 3°25'±1° | 3°27'±1° | 3°29'±1° | 3°32'±1° | 3°35'±1°
Camber angle*1(reference value) | -0°07'±1° | -0°08'±1°
Steering axis inclination (reference value) | 5°15' | 5°16'

  *1 :
Difference between left and right must not exceed 1°30'.

4SD 4WD

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Maximum steering angle | Inner | 36°±3°
Outer | 30°±3°
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Caster angle*1 (reference value) | 3°46'±1° | 3°48'±1° | 3°50'±1° | 3°51'±1° | 3°53'±1°
Camber angle*1(reference value) | -0°16'±1° | -0°17'±1°
Steering axis inclination (reference value) | 5°28' | 5°30'

  *1 :
Difference between left and right must not exceed 1°30'.

## Rear Suspension (Unloaded)

• Unloaded: Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.

4SD, 5HB

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Camber angle*1 | normal | -1°05'±1° | -1°07'±1° | -1°09'±1° | -1°11'±1° | -1°13'±1°
elevated*2 | -0°56'±1° | -0°58'±1° | -1°00'±1° | -1°02'±1° | -1°05'±1°
Thrust angle | 0°±0°48'

  *1 :
Difference between left and right must not exceed 1°30'.
  *2 :
Distance between wheel center and fender brim is following. L8, LF, L3: 401 mm {15.8 in} (reference value) MZR-CD (RF Turbo): 392 mm {15.4 in} (reference value)

WGN 2WD

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Camber angle*1 | normal | -0°59'±1° | -1°00'±1° | -1°02'±1° | -1°04'±1° | -1°06'±1°
elevated*2 | -0°52'±1° | -0°53'±1° | -0°55'±1° | -0°56'±1° | -0°58'±1°
Thrust angle | 0°±0°48'

  *1 :
Difference between left and right must not exceed 1°30'.
  *2 :
Distance between wheel center and fender brim is 407 mm {16.02 in} (reference value).

WGN 4WD

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Camber angle*1 | -0°55'±1° | -0°57'±1° | -0°59'±1° | -1°01'±1° | -1°03'±1°
Thrust angle | (degree) | 0°±0°48'

  *1 :
Difference between left and right must not exceed 1°30'.

4SD 4WD

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | (mm {in}) | Tire: 2±4 {0.08±0.16}, Rim inner: 1±3 {0.04±0.12}
(degree) | 0°11'±0°22'
Camber angle*1 | -1°28'±1° | -1°30'±1° | -1°33'±1° | -1°35'±1° | -1°37'±1°
Thrust angle | (degree) | 0°±0°48'

  *1 :
Difference between left and right must not exceed 1°30'.

## Wheel and Tire

European (L.H.D. U.K.) specs.

Item | Specification
--- | ---
Standard tire and wheel
Wheel | Size | 15 × 6J | 16 × 7J | 17 × 7J | 18 × 7J
Offset | (mm {in}) | 50 {1.97} | 55 {2.17}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Steel | Aluminum alloy
Tire | Size | 195/65R15 91V | 205/55R16 91V | 215/45R17 87W | 215/45R17 91W (reinforced) | Mazda6 MPS: 215/45R18 93Y Except Mazda6 MPS: 215/45R 18 89W
Air pressure (kPa {(kgf/cm2, bar), <psi>}) | Front | Up to 4 persons | 220 {(2.2, 2.2), <32>} | 2WD: 230 {(2.3, 2.3), <33>} 4WD: 250 {(2.5, 2.5), <36>} | Mazda6 MPS: 260 {(2.6, 2.6), <38>} Except Mazda6 MPS: 220 {(2.2, 2.2), <32>}
Full load | 240 {(2.4, 2.4), <35>} | 2WD: 240 {(2.4, 2.4), <35>} 4WD:250 {(2.5, 2.5), <36>} | Mazda6 MPS: 270 {(2.8, 2.7), <39>} Except Mazda6 MPS: 240 {(2.4, 2.4), <35>}
Rear | Up to 4 persons | 220 {(2.2, 2.2), <32>} | 2WD: 230 {(2.3, 2.3), <33>} 4WD: 250 {(2.5, 2.5), <36>} | Mazda6 MPS: 260 {(2.6, 2.6), <38>} Except Mazda6 MPS: 220 {(2.2, 2.2), <32>}
Full load | 300 {(3.1, 3.0), <44>} | 270 {(2.8, 2.7), <39>} | Mazda6 MPS: 290 {(2.9, 2.9), <42>} Except Mazda6 MPS: 270 {(2.8, 2.7), <39>}
Remaining tread | (mm {in}) | 1.6 {0.06}
Wheel and tire | Wheel and tire runout | Radial direction | 1.5 {0.06} max.
(mm {in}) | Lateral direction | 2.5 {0.10} max. | 2.0 {0.08} max.
Wheel imbalance | (g {oz}) | Knock-type*2: 9 {0.32} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max. | Adhesive-type*1: 10 {0.35} max. Knock-type*2: 6 {0.21} max.
Temporary spare tire
Wheel | Size | 15 × 4T | 17 × 4T
Offset | (mm {in}) | 40 {1.57}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Steel
Tire | Size | T115/70 D15 | 2WD: T115/70 D15 4WD: T135/90 D15 | Mazda6 MPS: T145/70 D17 Except Mazda6 MPS: T125/70 D17
Air pressure | (kPa {(kgf/cm2, bar), <psi>}) | 420 {(4.2, 4.2), <60>}
Wheel and tire | Wheel and tire runout | Radial direction | 2.0 {0.08} max.
(mm {in}) | Lateral direction | 2.5 {0.10} max.

  *1 :
Total weight exceeds 160 g {5.65 oz} .
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.

Australian specs

Item | Specification
--- | ---
Standard tire and wheel
Wheel | Size | 15 × 6J | 16 × 7J | 17 × 7J | 18 × 7J
Offset | (mm {in}) | 50 {1.97} | 55 {2.17}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Steel | Aluminum alloy
Tire | Size | 195/65R15 91V | 205/55R16 91V | 215/45R17 87W | 215/45R18 89W
Air pressure (kPa {bar} <psi>) | Front | 220 {2.2} <32> | L3 ATX: 230 {2.3} <33> | 260 {(2.6), <38>}
Rear
Remaining tread | (mm {in}) | 1.6 {0.06}
Wheel and tire | Wheel and tire runout | Radial direction | 1.5 {0.06} max.
(mm {in}) | Lateral direction | 2.5 {0.10} max. | 2.0 {0.08} max.
Wheel imbalance | (g {oz}) | Knock-type*2: 9 {0.32} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max. | Adhesive-type*1: 10 {0.35} max. Knock-type*2: 6 {0.21} max.
Temporary spare tire
Wheel | Size | - | 17 × 4T
Offset | (mm {in}) | - | 40 {1.57}
Pitch circle diameter | (mm {in}) | - | 114.3 {4.50}
Material | - | Steel
Tire | Size | - | T145/70 D17
Air pressure | (kPa {bar} <psi>) | - | 420 {4.2} <60>
Wheel and tire | Wheel and tire runout | Radial direction | - | 2.0 {0.08} max.
(mm {in}) | Lateral direction | - | 2.5 {0.10} max.

  *1 :
Total weight exceeds 160 g {5.65 oz} .
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.

General (L.H.D. R.H.D.) specs

Item | Specification
--- | ---
Standard tire and wheel
Wheel | Size | 15 × 6J | 16 × 7J | 17 × 7J
Offset | (mm {in}) | 50 {1.97} | 55 {2.17}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Steel | Aluminum alloy
Tire | Size | 195/65R15 91V | 205/55R16 91V | 215/45R17 87W | 215/45R17 91W (reinforced)
Air pressure (kPa {(kgf/cm2, bar), <psi>}) | Front | Up to 4 persons | 220 {(2.2, 2.2), <32>}
Full load | 240 {(2.4, 2.4), <35>}
Rear | Up to 4 persons | 220 {(2.2, 2.2), <32>}
Full load | 300 {(3.1, 3.0), <44>} | 270 {(2.8, 2.7), <39>}
Remaining tread | (mm {in}) | 1.6 {0.06}
Wheel and tire | Wheel and tire runout | Radial direction | 1.5 {0.06} max.
(mm {in}) | Lateral direction | 2.5 {0.10} max. | 2.0 {0.08} max.
Wheel imbalance | (g {oz}) | Knock-type*2: 9 {0.32} max. | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 11 {0.39} max. Knock-type*2: 7 {0.25} max.
Temporary spare tire (General (L.H.D.) specs.)
Wheel | Size | 15 × 4T
Offset | (mm {in}) | 40 {1.57}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Steel
Tire | Size | T115/70 D15
Air pressure | (kPa {(kgf/cm2, bar), <psi>}) | 420 {(4.2, 4.2), <60>}
Wheel and tire | Wheel and tire runout | Radial direction | 2.0 {0.08} max.
(mm {in}) | Lateral direction | 2.5 {0.10} max.

  *1 :
Total weight exceeds 160 g {5.65 oz} .
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.

Item | Specification
--- | ---
Front upper arm rotation torque | 1.5 N·m {15.0 kgf·cm, 13.2 in·lbf} max.
Front lower arm (front) rotation torque | 1.18-2.23 N·m {12.1-22.7 kgf·cm, 10.5-19.7 in·lbf}
Front lower arm (rear) rotation torque | 1.00-2.22 N·m {10.2-22.6 kgf·cm, 8.86-19.6 in·lbf}
Front stabilizer control link starting torque | 0.2-0.8 N·m {2.1-8.1 kgf·cm, 1.8-7.0 in·lbf}
Rear stabilizer control link starting torque | 0.23-0.47 N·m {2.4-4.7 kgf·cm, 2.1-4.1 in·lbf}