#
RECLINER MOTOR REMOVAL/INSTALLATION

id091300804000

1. Disconnect the negative battery cable.

2. Remove the driver's side front seat. (See FRONT SEAT REMOVAL/INSTALLATION.)

3. Remove the front cover (No.1, No.2) and side cover. (See FRONT SEAT DISASSEMBLY/ASSEMBLY.)

4. Remove in the order indicated in the table.

1 | Bolt
2 | Connector
3 | Recliner motor

5. Install in the reverse order of removal.