#
REAR DRAIN HOSE INSTALLATION

id091500801600

  Caution

  • If the rear drain hose is pinched or bent anywhere, the water in the hose may not discharge and enter the inside of the vehicle. During and after installation of the trims and the headliner, always make sure there is no interference with the rear drain hose. Fix any problem if found.

1. Apply soapy water to the rear drain hose inserting area.

2. Insert one end (the wider side) of the rear drain hose into the sunroof frame.

3. Install the rear drain hose to the clips parallel to the pillar and free of slack.

4. Insert the rear drain hose joint into the rear pillar inner hole.

5. Install the trunk side trim.(See TRUNK SIDE TRIM REMOVAL/INSTALLATION [4SD, 5HB].)

6. Install the trunk side upper trim(5HB, WGN).(See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [5HB].)(See TRUNK SIDE UPPER TRIM REMOVAL/INSTALLATION [WGN].)

7. Install the headliner.(See HEADLINER REMOVAL/INSTALLATION [4SD, 5HB].)(See HEADLINER REMOVAL/INSTALLATION [WGN].)

8. Install the net anchor (WGN).

9. Install the assist handle.(See ASSIST HANDLE REMOVAL/INSTALLATION.)

10. Install the sunvisors.(See (SUNVISOR REMOVAL/INSTALLATION.)

11. Install the cargo compartment light (WGN).(See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION [WGN].)

12. Install the rear map light.(See REAR MAP LIGHT REMOVAL/INSTALLATION.)

13. Install the front map light.(See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

14. Install the D-pillar trims (WGN).(See D-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

15. Install the C-pillar trims.(See C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB].)(See C-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

16. Install the B-pillar upper trims.(See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

17. Install the A-pillar trims.(See A-PILLAR TRIM INSTALLATION.)

18. Install the sunroof seaming welt.