#
REAR AUTO LEVELING SENSOR INSPECTION [4WD]

id0918004741a4

1. Connect the three dry cell batteries in series.

2. Connect the positive pole of the battery to auto leveling sensor terminal A, and the negative pole to terminal D.

3. Connect the tester as shown in the figure.

4. Measure the voltage while the link is moved up and down slowly.

  • If not as indicated in the table, replace the auto leveling sensor.

Link angle (vehicle height) | Voltage (V)
--- | ---
+35°(High) | 4.059
0° | 2.237
-35°(Low) | 0.468