#
POWER WINDOW SYSTEM WIRING DIAGRAM

id091200006600

## With Auto-Open/Close Function For All Windows

### Power window main switch

.

1 | Power window main switch
2 | Power window motor (driver's side)
3 | Close
4 | Open
5 | Auto
6 | Power-cut switch
7 | Conjunction circuit
8 | Close relay
9 | Open relay
10 | Hall effect switch 1
11 | Hall effect switch 2
12 | To power outside mirror switch

### Power window subswitch

.

1 | Power window subswitch
2 | Power window motor
3 | Close
4 | Open
5 | Auto
6 | Close relay
7 | Open relay
8 | Hall effect switch 1
9 | Hall effect switch 2
10 | To power window main switch A
11 | To power window main switch B

## With Auto-Open/Close Function For Driver's side

.

1 | Power window main switch
2 | Manual close
3 | Manual open
4 | Auto
5 | Power-cut switch
6 | Close
7 | Open
8 | Close relay
9 | Open relay
10 | Power window subswitch
11 | Front power window motor (Driver's side)
12 | Hall effect switch 1
13 | Hall effect switch 2
14 | Front power window motor (Passenger's side)
15 | Rear power window motor (Right side)
16 | Rear power window motor (Left side)
17 | Door switch
18 | To power outside mirror switch
19 | Vehicle with IG-OFF timer
20 | Vehicle without IG-OFF timer