#
GLOW PLUG INSPECTION [MZR-CD (RF Turbo)]

id0113f1804300

  Note

  • Perform the following test only when directed.

1. Remove the glow plug lead. (See GLOW PLUG REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Measure the resistance between the glow plug terminal and the cylinder head (body ground) using an ohmmeter.

  • If not as specified, replace the glow plug. (See GLOW PLUG REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

Resistance (Reference value)

  Approx. 0.6 ohms [20°C {68°F}]

3. Install the glow plug lead.